
**ONE-X SETTINGS**

There are 2 screens to set, the other you can leave as is. Launch the One-X application after installing and set the telephony screen and the Dialing rules screen, then save.


**Under One-X select settings:**



Select Telephony and set your **extension** and **password** of 1111

Add the server: 198.248.193.106.

(If it asks for a proxy, ignore this and move to the next screen, then save. After save, go back into



**Next:**

Select Dialing rules and set the rules as diplayed below.

